
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 11:42:13.899
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.3 Hz, Target= 0.3 Hz, After= 1.0 Hz
Iteration 2: FWHM Before= 1.0 Hz, Target= 0.3 Hz, After= 0.6 Hz
Iteration 3: FWHM Before= 0.6 Hz, Target= 0.3 Hz, After= 0.8 Hz
Iteration 4: FWHM Before= 0.8 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.403


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-18
Z2	-25
Z3	+65
Z4	+579
Z5	-348
Z6	-3654
Z7	+2067
Z8	+18003
X	+9
XZ	+1
Y	+8
YZ	+8

duration = 1 min 28 sec
completed successfully
finished Tue Dec 21 11:43:40 2021


========================================================================
