
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 12:58:11.080
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 2.1 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 3: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.495


Performing tune after shimming

NOTE: The lock signal appears to be unstable. This affects the performance of the tune algorithm! 

tune lock level increase = 1.0

shim changes: 
Z	+29
Z2	+8
Z3	+80
Z4	+116
Z5	-276
Z6	-1178
Z7	+440
Z8	+8499
X	+6
XZ	+31
Y	+55
YZ	+32

duration = 1 min 49 sec
completed successfully
finished Tue Dec 21 12:59:58 2021


========================================================================
