
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 12:33:39.670
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.3 Hz, Target= 0.2 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration 3: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.8 Hz
Iteration 4: FWHM Before= 0.8 Hz, Target= 0.2 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.394


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+54
Z2	-36
Z3	+16
Z4	+749
Z5	-173
Z6	-4088
Z7	+611
Z8	+17640
X	+14
XZ	+8
Y	+57
YZ	-16

duration = 1 min 30 sec
completed successfully
finished Wed Dec 22 12:35:08 2021


========================================================================
