EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
T_NAME		Date_
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 50000000
		REL	"Date_=itodate(DATE)"
		INV_REL	"DATE=datetoi(Date_,DATE)"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		Time
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"Time=itotime(DATE)"
		INV_REL	"DATE=timetoi(Time,DATE)"
		FORMAT	"%14.2f"
		TEXT	" "
END
NAME		INSTRUM
		TEXT	" "
END
NAME		PROBHD
		FORMAT	"%14.14s"
		TEXT	" "
END
NAME		PULPROG
		TEXT	" "
END
NAME		TD
		TEXT	" "
END
NAME		SOLVENT
		TEXT	" "
END
NAME		NS
		TEXT	" "
END
NAME		DS
		TEXT	" "
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e8
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.3f Hz"
		TEXT	" "
END
T_NAME          FIDRES
                TYPE    R32
                CLASS   ACQU
                SUBRANGE 0.0 100000
                REL     "FIDRES=SW*SFO1/TD"
                INV_REL "TD = nextpow(SW*SFO1/FIDRES)"
		UNIT	"Hz"
		FORMAT	"%14.6f Hz"
		TEXT	" "
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
		TEXT	" "
END
NAME		RG
		TEXT	" "
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3lf usec"
		TEXT	" "
END
NAME		DE
		FORMAT	"%14.2f usec"
		TEXT	" "
END
NAME		TE
		FORMAT	"%14.1f K"
		TEXT	" "
END
T_NAME		CEN_HC1
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"CEN_HC1=C13_90-H1_90"
		INV_REL	"D[0]=CEN_HC1"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=d13+in0/2"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"D2=D[2]"
		INV_REL	"D[2]=D2"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		D4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"D4=D[4]"
		INV_REL	"D[4]=D4"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		d6
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d6=H1_90"
		INV_REL	"D[0]=d6"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d7
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d7=C13_90"
		INV_REL	"D[0]=d7"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=100m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d12
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d12=10u"
		INV_REL	"D[0]=d12"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d13
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d13=5u"
		INV_REL	"D[0]=d13"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d14
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d14=60u"
		INV_REL	"D[0]=d14"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d16
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d16=300u"
		INV_REL	"D[0]=d16"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d31
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d31=2*(TAUA2+TAUA4+TAUA5+GRAD2+GRAD4+GRAD5+GRAD6)+GRAD1+GRAD3+GRAD7+TAUB"
		INV_REL	"D[0]=d31"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		IN0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"IN0=IN[0]"
		INV_REL	"IN[0]=IN0"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		L4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"L4=L[4]"
		INV_REL	"L[4]=L4"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P3=P[3]"
		INV_REL	"P[3]=P3"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		p19
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"p19=91.65u"
		INV_REL	"D[0]=p19"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		TAUA2
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"TAUA2=d2-GRAD2-d16-d13"
		INV_REL	"D[0]=TAUA2"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		TAUA4
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"TAUA4=d4-GRAD4-d16-d13"
		INV_REL	"D[0]=TAUA4"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		TAUA5
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"TAUA5=d2-GRAD5-d16-d13"
		INV_REL	"D[0]=TAUA5"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		TAUB
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"TAUB=d16+GRAD3+H1_180+d13*5"
		INV_REL	"D[0]=TAUB"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
HEADER		"============ CHANNEL f1 ============="
T_NAME		H1_90
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"H1_90=p1"
		INV_REL	"D[0]=H1_90"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		H1_180
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"H1_180=H1_90*2"
		INV_REL	"D[0]=H1_180"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
NAME		NUC1
		TEXT	" "
END
T_NAME		PL1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL1=PL[1]"
		INV_REL	"PL[1]=PL1"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	" "
END
HEADER		"============ CHANNEL f2 ============="
T_NAME		C13_180
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"C13_180=C13_90*2"
		INV_REL	"D[0]=C13_180"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		C13_90
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"C13_90=p3"
		INV_REL	"D[0]=C13_90"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
NAME		CPDPRG3
		TEXT	" "
END
NAME		NUC2
		TEXT	" "
END
T_NAME		PCPD2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1000000 1000000
		REL	"PCPD2=PCPD[2]"
		INV_REL	"PCPD[2]=PCPD2"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		PL2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL2=PL[2]"
		INV_REL	"PL[2]=PL2"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
T_NAME		PL3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL3=PL[3]"
		INV_REL	"PL[3]=PL3"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
T_NAME		PL13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL13=PL[13]"
		INV_REL	"PL[13]=PL13"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
NAME		SFO2
		FORMAT	"%14.7f MHz"
		TEXT	" "
END
HEADER		"============ GRADIENT CHANNEL ========"
NAME		GPNAM1
		TEXT	" "
END
NAME		GPNAM2
		TEXT	" "
END
NAME		GPNAM3
		TEXT	" "
END
NAME		GPNAM4
		TEXT	" "
END
NAME		GPNAM5
		TEXT	" "
END
NAME		GPNAM6
		TEXT	" "
END
NAME		GPNAM7
		TEXT	" "
END
T_NAME		GPX1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX1=GPX[1]"
		INV_REL	"GPX[1]=GPX1"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX2=GPX[2]"
		INV_REL	"GPX[2]=GPX2"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX3=GPX[3]"
		INV_REL	"GPX[3]=GPX3"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX4=GPX[4]"
		INV_REL	"GPX[4]=GPX4"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX5=GPX[5]"
		INV_REL	"GPX[5]=GPX5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX6=GPX[6]"
		INV_REL	"GPX[6]=GPX6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX7=GPX[7]"
		INV_REL	"GPX[7]=GPX7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY1=GPY[1]"
		INV_REL	"GPY[1]=GPY1"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY2=GPY[2]"
		INV_REL	"GPY[2]=GPY2"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY3=GPY[3]"
		INV_REL	"GPY[3]=GPY3"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY4=GPY[4]"
		INV_REL	"GPY[4]=GPY4"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY5=GPY[5]"
		INV_REL	"GPY[5]=GPY5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY6=GPY[6]"
		INV_REL	"GPY[6]=GPY6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY7=GPY[7]"
		INV_REL	"GPY[7]=GPY7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ1=GPZ[1]"
		INV_REL	"GPZ[1]=GPZ1"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ2=GPZ[2]"
		INV_REL	"GPZ[2]=GPZ2"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ3=GPZ[3]"
		INV_REL	"GPZ[3]=GPZ3"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ4=GPZ[4]"
		INV_REL	"GPZ[4]=GPZ4"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ5=GPZ[5]"
		INV_REL	"GPZ[5]=GPZ5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ6=GPZ[6]"
		INV_REL	"GPZ[6]=GPZ6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ7=GPZ[7]"
		INV_REL	"GPZ[7]=GPZ7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GRAD1
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD1=400u"
		INV_REL	"D[0]=GRAD1"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD2
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD2=400u"
		INV_REL	"D[0]=GRAD2"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD3
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD3=720u"
		INV_REL	"D[0]=GRAD3"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD4
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD4=250u"
		INV_REL	"D[0]=GRAD4"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD5
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD5=250u"
		INV_REL	"D[0]=GRAD5"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD6
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD6=p19"
		INV_REL	"D[0]=GRAD6"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		GRAD7
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"GRAD7=4.0m"
		INV_REL	"D[0]=GRAD7"
		UNIT	"usec"
		TEXT	" "
		FORMAT	"%14.2f usec"
		NONEDIT
END
