# 1 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu"
;HMQCosy written by Kaifeng Hu, May, 2010
;avance-version (07/04/04)
;HMQCosy constant time version
;2D H-1/X correlation via double inept transfer
;phase sensitive using Echo/Antiecho-TPPI gradient selection
;with decoupling during acquisition
;using trim pulses in inept transfer
;
;$CLASS=HighRes
;$DIM=2D
;$TYPE=
;$SUBTYPE=
;$COMMENT=


# 1 "/opt/topspin216/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance3.incl
;   for AV III
;
;avance-version (07/12/14)
;
;$CLASS=HighRes Incl
;$COMMENT=





























































































































































;$Id: Avance3.incl,v 1.6.2.2 2007/12/14 16:06:46 ber Exp $
# 16 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu" 2

# 1 "/opt/topspin216/exp/stan/nmr/lists/pp/Grad.incl" 1
;Grad2.incl  -  include file for Gradient Spectroscopy
;   for 1
;
;avance-version (07/01/17)
;
;$CLASS=HighRes Incl
;$COMMENT=



















define list<gradient> EA=<EA>



;$Id: Grad2.incl,v 1.12 2007/01/22 14:22:35 ber Exp $
# 17 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu" 2

# 1 "/opt/topspin216/exp/stan/nmr/lists/pp/Delay.incl" 1
;Delay.incl  -  include file for commonly used delays
;
;version 00/02/07
;
;$CLASS=HighRes Incl
;$COMMENT=


;general delays

define delay DELTA
define delay DELTA1
define delay DELTA2
define delay DELTA3
define delay DELTA4
define delay DELTA5
define delay DELTA6
define delay DELTA7
define delay DELTA8

define delay TAU
define delay TAU1
define delay TAU2
define delay TAU3
define delay TAU4
define delay TAU5


;delays for centering pulses

define delay CEN_HN1
define delay CEN_HN2
define delay CEN_HN3
define delay CEN_HC1
define delay CEN_HC2
define delay CEN_HC3
define delay CEN_HC4
define delay CEN_HP1
define delay CEN_HP2
define delay CEN_CN1
define delay CEN_CN2
define delay CEN_CN3
define delay CEN_CN4
define delay CEN_CP1
define delay CEN_CP2


;loop counters

define loopcounter COUNTER
define loopcounter SCALEF
define loopcounter FACTOR1
define loopcounter FACTOR2
define loopcounter FACTOR3



;$Id: Delay.incl,v 1.12 2005/11/10 12:16:58 ber Exp $
# 18 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu" 2

;#define LABEL_CN
;#define TANGO

"p2=p1*2"
"p4=p3*2"
"d4=1s/(cnst2*4)"
"d11=30m"
"d13=4u"






"in0=inf1/4"
"in9=in0"

"DELTA=p16+d16+d13"
"DELTA1=DELTA-4u"

"d0=d6/4"
"d9=d6/4-DELTA"


# 1 "mc_line 43 file /opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu expanding definition part of mc command before ze"
define delay MCWRK
define delay MCREST
define loopcounter ST1CNT
"ST1CNT = td1 / (2)"
"MCWRK = 0.142857*d1"
"MCREST = d1 - d1"
    dccorr
# 43 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu"
1 ze
# 1 "mc_line 43 file /opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu expanding definition of mc command after ze"
# 44 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu"
  d11 pl12:f2
# 1 "mc_line 45 file /opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu expanding start label for mc command"
2 MCWRK  do:f2
LBLSTS1, MCWRK  * 5
LBLF1, MCWRK 
  MCREST
# 46 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu"
3 d11 







  (p1 ph1)

  d4 pl2:f2
  (center (p2 ph1) (p4 ph1):f2 )
  d4 setnmr3|0 setnmr0|34|32|33 ctrlgrad 0
;  p28 ph1
;  d13
  (p3 ph3):f2 ;(p1 ph2)
  d0 




  (p2 ph5)


  d0

  (p4 ph4):f2
  d9
; gradient selection here
  d13
  p16:gp1*EA
  d16 



  (p2 ph7)

  d13
  p16:gp1*EA
  d16  
  d9
  (p3 ph4):f2   ; end of MQ

  d4
  (center (p2 ph1) (p4 ph1):f2 )
  d4
  p1 ph6   ;COSY transfer pulse
  d13
  p16:gp2
  d16
  (p2 ph1)
  DELTA1 pl12:f2
  4u setnmr3^0 setnmr0^34^32^33 ctrlgrad 7
  go=2 ph31 cpd2:f2
# 1 "mc_line 100 file /opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu expanding mc command in line"
  MCWRK  do:f2 wr #0 if #0 zd igrad EA
  lo to LBLSTS1 times 2
  MCWRK dd0  MCWRK  id9  MCWRK  ip3*2  MCWRK  ip6*2  MCWRK  ip31*2
  lo to LBLF1 times ST1CNT
  MCWRK
# 102 "/opt/topspin216/exp/stan/nmr/lists/pp/user/hmqcosyetgpct2.khu"
exit
   

ph1=0 
ph2=1
ph3=0 2
ph4=0 0 0 0 2 2 2 2
ph5=0 0 2 2
ph6=1 1 3 3
ph7=2 2 0 0
ph8=2
ph31=0 2 0 2 2 0 2 0
  

;pl1 : f1 channel - power level for pulse (default)
;pl2 : f2 channel - power level for pulse (default)
;pl3 : f3 channel - power level for pulse (default)
;pl12: f2 channel - power level for CPD/BB decoupling
;p1 : f1 channel -  90 degree high power pulse
;p2 : f1 channel - 180 degree high power pulse
;p3 : f2 channel -  90 degree high power pulse
;p4 : f2 channel - 180 degree high power pulse
;p16: homospoil/gradient pulse
;p22: f3 channel - 180 degree high power pulse
;p28: f1 channel - trim pulse
;d0 : incremented delay (2D)                  [3 usec]
;d1 : relaxation delay; 1-5 * T1
;d4 : 1/(4J)XH
;d6 : it is the constant time period, for c13 labeled sample, set to be 28ms
;d11: delay for disk I/O                             [30 msec]
;d13: short delay                                    [4 usec]
;d16: delay for homospoil/gradient recovery
;cnst2: = J(XH)
;inf1: 1/SW(X) = 2 * DW(X)
;in0: 1/(2 * SW(X)) = DW(X)
;nd0: 4
;NS: 1 * n
;DS: >= 16
;td1: number of experiments
;FnMODE: echo-antiecho
;cpd2: decoupling according to sequence defined by cpdprg2
;pcpd2: f2 channel - 90 degree pulse for decoupling sequence


;use gradient ratio:	gp 1 : gp 2
;		        40 : 20.12    for C-13 positive

;for z-only gradients:
;gpz1: 40%
;gpz2: 20.1% for C-13, 8.1% for N-15

;use gradient files:   
;gpnam1: SINE.100
;gpnam2: SINE.100

                                          ;preprocessor-flags-start
;LABEL_CN: for C-13 and N-15 labeled samples start experiment with 
;             option -DLABEL_CN (eda: ZGOPTNS)
                                          ;preprocessor-flags-end



;$Id: hsqcetgp,v 1.4 2007/04/11 13:34:30 ber Exp $
