cq-00509_AutoRun_Report.20120604_1010.txt
Status Report for Automated Sample Data Collection
Initiated - 4-6-2012, 10:10
# Host = kerry.nmrfam.wisc.edu


info:
cq-00509_CDCl3_6-4-2012
  #cq-00509 in CDCl3 at position 101
  #Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCGPND,COSY45SW,HSQC_TOCSY_ADIA

- instrument initialization - passed
- loading sample position 101 - passed
- sample solvent lock - passed
- tuning probe channels - passed
- topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters - passed
- prosol parameters loaded
- creating exp 2 with metabTOCSY parameters - passed
- prosol parameters loaded
- creating exp 3 with C13CPD parameters - passed
- prosol parameters loaded
- creating exp 4 with C13DEPT90 parameters - passed
- prosol parameters loaded
- creating exp 5 with C13DEPT135_MMCD parameters - passed
- prosol parameters loaded
- creating exp 6 with HSQCETGP parameters - passed
- prosol parameters loaded
- creating exp 7 with HSQCETGP parameters - passed
- prosol parameters loaded
- creating exp 8 with HMBCGPND parameters - passed
- prosol parameters loaded
- creating exp 9 with COSY45SW parameters - passed
- prosol parameters loaded
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
- prosol parameters loaded
- experiment folders set up - passed
# Exp 1 started 10:17_20120604
- ZGCPPR (zgcppr)
- optimizing receiver gain - passed
- receiver gain set to 36
# Exp 1 ended
  10:18_20120604 - passed
- 1H adaptive offset determined = 4.7498
- 1H adaptive SW determined = 10.2985
# Exp 2 started 10:18_20120604
- metabTOCSY (mlevph)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 2 ended
  11:38_20120604 - passed
# Exp 3 started 11:38_20120604
- C13CPD (zgpg30)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 3 ended
  12:32_20120604 - passed
# Exp 4 started 12:32_20120604
- C13DEPT90 (dept90)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 4 ended
  12:46_20120604 - passed
# Exp 5 started 12:46_20120604
- C13DEPT135_MMCD (deptsp135)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 5 ended
  13:00_20120604 - passed
- 13C adaptive offset determined = 45.6875
- 13C adaptive SW determined = 73.1122
# Exp 6 started 13:00_20120604
- HSQCETGP (hsqcetgp)
- 1 SW changed to 73.1122
- 2 SW changed to 10.2985
- 1H offset changed to 4.7498
- 13C offset changed to 45.6875
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 6 ended
  13:14_20120604 - passed
# Exp 7 started 13:14_20120604
- HSQCETGP (hsqcetgp)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 7 ended
  13:29_20120604 - passed
# Exp 8 started 13:29_20120604
- HMBCGPND (hmbcgpndqf)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 8 ended
  14:02_20120604 - passed
# Exp 9 started 14:02_20120604
- COSY45SW (cosyqf45)
- optimizing receiver gain - passed
- receiver gain set to 80.6
# Exp 9 ended
  14:40_20120604 - passed
# Exp 10 started 14:40_20120604
- HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 10 ended
  15:58_20120604 - passed

Ended - 4-6-2012, 15:58

