NMRbot_cq_07330_SampleReport.20130527_2100.txt
Status Report for Automated Sample Data Collection
# Host = kerry.nmrfam.wisc.edu

# Initiated - 20130527_2100

- info:
cq_07330.CDCl3.202.20130527 = cq_07330 in CDCl3 at position 202
   Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 202 - passed
- sample solvent lock - passed
- tuning probe channels - passed
- topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters - passed
- prosol parameters loaded
- creating exp 2 with metabTOCSY parameters - passed
- prosol parameters loaded
- creating exp 3 with C13CPD parameters - passed
- prosol parameters loaded
- creating exp 4 with C13DEPT90 parameters - passed
- prosol parameters loaded
- creating exp 5 with C13DEPT135_MMCD parameters - passed
- prosol parameters loaded
- creating exp 6 with HSQCETGP parameters - passed
- prosol parameters loaded
- creating exp 7 with HSQCETGP parameters - passed
- prosol parameters loaded
- creating exp 8 with HMBCETGPL3ND parameters - passed
- prosol parameters loaded
- creating exp 9 with COSY45SW parameters - passed
- prosol parameters loaded
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
- prosol parameters loaded
- experiment folders set up - passed
# Exp 1 started - 20130527_2108
- ZGCPPR (zgcppr)
- optimizing receiver gain - passed
- receiver gain set to 22.6
# Exp 1 ended - 20130527_2109 - passed
- 1H adaptive offset determined = 4.7498
- 1H adaptive SW determined = 10.2335
# Exp 2 started - 20130527_2109
- metabTOCSY (mlevph)
- optimizing receiver gain - passed
- receiver gain set to 32
# Exp 2 ended - 20130527_2228 - passed
# Exp 3 started - 20130527_2228
- C13CPD (zgpg30)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 3 ended - 20130527_2323 - passed
# Exp 4 started - 20130527_2323
- C13DEPT90 (dept90)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 4 ended - 20130527_2336 - passed
# Exp 5 started - 20130527_2336
- C13DEPT135_MMCD (deptsp135)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 5 ended - 20130527_2350 - passed
- 13C adaptive offset determined = 97.2214
- 13C adaptive SW determined = 176.3251
# Exp 6 started - 20130527_2350
- HSQCETGP (hsqcetgp)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 6 ended - 20130528_0005 - passed
# Exp 7 started - 20130528_0005
- HSQCETGP (hsqcetgp)
- 1 SW changed to 176.3251
- 2 SW changed to 10.2335
- 1H offset changed to 4.7498
- 13C offset changed to 97.2214
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 7 ended - 20130528_0019 - passed
# Exp 8 started - 20130528_0019
- HMBCETGPL3ND (hmbcetgpl3nd)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 8 ended - 20130528_0101 - passed
# Exp 9 started - 20130528_0101
- COSY45SW (cosyqf45)
- optimizing receiver gain - passed
- receiver gain set to 40.3
# Exp 9 ended - 20130528_0140 - passed
# Exp 10 started - 20130528_0140
- HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 10 ended - 20130528_0258 - passed

# cq_07330 Experiment Set Ended - 20130528_0258

