NMRbot_cq_18892_SampleReport.20131002_0752.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## Initiated - 20131002_0752 ##

- info:
  cq_18892 in D2O at position 203
  foldername => cq_18892.D2O.203.20131001
  Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 203 - passed
-   sample solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
-   determined 1H offset = 4.6991
- creating exp 1 with ZGCPPR parameters - passed
-   prosol parameters loaded
-   NS changed to 40
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 40.3
- creating exp 2 with metabTOCSY parameters - passed
-   prosol parameters loaded
-   NS changed to 40
-   1H offset changed to 4.6991
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD parameters - passed
-   prosol parameters loaded
-   NS changed to 5120
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters - passed
-   prosol parameters loaded
-   NS changed to 1280
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters - passed
-   prosol parameters loaded
-   NS changed to 1280
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 10
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 10
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND parameters - passed
-   prosol parameters loaded
-   NS changed to 20
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters - passed
-   prosol parameters loaded
-   NS changed to 40
-   1H offset changed to 4.6991
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 71.8
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
-   prosol parameters loaded
-   NS changed to 40
-   1H offset changed to 4.6991
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
-   dims 1- F1 1H, SW 16.0307
- start 20131002_0805
- end   20131002_0808 - passed
-   1H adaptive offset determined = 4.6991
-   1H adaptive SW determined = 9.4640
# Exp 2 - metabTOCSY (mlevph)
-   dims 2- F1 1H, SW 10.2073; F2 1H, SW 10.2073
- start 20131002_0808
- end   20131002_1440 - passed
# Exp 3 - C13CPD (zgpg30)
-   dims 1- F1 13C, SW 236.7742
- start 20131002_1440
- end   20131002_1910 - passed
# Exp 4 - C13DEPT90 (dept90)
-   dims 1- F1 13C, SW 236.7742
- start 20131002_1910
- end   20131002_2018 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
-   dims 1- F1 13C, SW 236.7742
- start 20131002_2018
- end   20131002_2125 - passed
-   13C adaptive offset determined = 58.9834
-   13C adaptive SW determined = 98.2707
# Exp 6 - HSQCETGP (hsqcetgp)
-   dims 2- F1 13C, SW 165.6393; F2 1H, SW 13.3375
- start 20131002_2125
- end   20131002_2234 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-   dims 2- F1 13C, SW 165.6393; F2 1H, SW 13.3375
-   F1 SW changed to 98.2707
-   F2 SW changed to 9.4640
-   F1 1H offset changed to 4.6991
-   F2 13C offset changed to 58.9834
- start 20131002_2234
- end   20131002_2344 - passed
# Exp 8 - HMBCETGPL3ND (hmbcetgpl3nd)
-   dims 2- F1 13C, SW 221.8327; F2 1H, SW 12.0230
- start 20131002_2344
- end   20131003_0311 - passed
# Exp 9 - COSY45SW (cosyqf45)
-   dims 2- F1 1H, SW 10.3125; F2 1H, SW 10.3125
- start 20131003_0312
- end   20131003_0621 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
-   dims 2- F1 13C, SW 165.6580; F2 1H, SW 11.9655
- start 20131003_0621
- end   20131003_1247 - passed

## cq_18892 Experiment Set Ended - 20131003_1247 ##

