cq_01653_AutoRun_Report.20121209_0031.txt
Status Report for Automated Sample Data Collection
Initiated - 9-12-2012, 0:31
# Host = kerry.nmrfam.wisc.edu


info:
cq_01653_D2O_12-7-2012
  #cq_01653 in D2O at position 106
  #Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCGPND,COSY45SW,HSQC_TOCSY_ADIA

- instrument initialization - passed
- loading sample position 106 - passed
- sample solvent lock - passed
- tuning probe channels - passed
- topshim tuneb tunea - passed
- determined 1H offset = 4.6994
- creating exp 1 with ZGCPPR parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- creating exp 2 with metabTOCSY parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- 1H offset changed to 4.6994
- creating exp 3 with C13CPD parameters - passed
- prosol parameters loaded
- creating exp 4 with C13DEPT90 parameters - passed
- prosol parameters loaded
- creating exp 5 with C13DEPT135_MMCD parameters - passed
- prosol parameters loaded
- creating exp 6 with HSQCETGP parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- creating exp 7 with HSQCETGP parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- creating exp 8 with HMBCGPND parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- creating exp 9 with COSY45SW parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- 1H offset changed to 4.6994
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
- prosol parameters loaded
- 1H offset changed to 4.6994
- experiment folders set up - passed
# Exp 1 started 00:40_20121209
- ZGCPPR (zgcppr)
- optimizing receiver gain - passed
- receiver gain set to 45.2
# Exp 1 ended
  00:41_20121209 - passed
- 1H adaptive offset determined = 4.6994
- 1H adaptive SW determined = 9.4656
# Exp 2 started 00:41_20121209
- metabTOCSY (mlevph)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 2 ended
  02:00_20121209 - passed
# Exp 3 started 02:00_20121209
- C13CPD (zgpg30)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 3 ended
  02:55_20121209 - passed
# Exp 4 started 02:55_20121209
- C13DEPT90 (dept90)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 4 ended
  03:09_20121209 - passed
# Exp 5 started 03:09_20121209
- C13DEPT135_MMCD (deptsp135)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 5 ended
  03:22_20121209 - passed
- 13C adaptive offset determined = 86.3454
- 13C adaptive SW determined = 152.9965
# Exp 6 started 03:22_20121209
- HSQCETGP (hsqcetgp)
- 1 SW changed to 152.9965
- 2 SW changed to 9.4656
- 1H offset changed to 4.6994
- 13C offset changed to 86.3454
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 6 ended
  03:37_20121209 - passed
# Exp 7 started 03:37_20121209
- HSQCETGP (hsqcetgp)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 7 ended
  03:51_20121209 - passed
# Exp 8 started 03:51_20121209
- HMBCGPND (hmbcgpndqf)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 8 ended
  04:24_20121209 - passed
# Exp 9 started 04:24_20121209
- COSY45SW (cosyqf45)
- optimizing receiver gain - passed
- receiver gain set to 71.8
# Exp 9 ended
  05:02_20121209 - passed
# Exp 10 started 05:02_20121209
- HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- optimizing receiver gain - passed
- receiver gain set to 203
# Exp 10 ended
  06:21_20121209 - passed

Ended - 9-12-2012, 6:21

